PTD6 button

PTB0 white analogue input to MCU - measure IR brightness

PTB8 blue digital output from MCU - switch on IR emitter

PTA4 audio PWM

PTA2 audio signal